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	APPLICATION DATA SHEET:  DENSITY / MASSFLOW UPGRADES
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	Quote Reference:
	[bookmark: Text10]     
	
	Tag:
	[bookmark: Text11]     
	

	Customer:
	[bookmark: Text2]     
	
	End-User:
	[bookmark: Text12][bookmark: Text4]     
	

	Fax No:
	[bookmark: Text3]     
	
	Date:
	[bookmark: Text5]     
	

	

	In order to evaluate the application and to ensure that any equipment subsequently purchased will be compatible with the process plant, certain minimum data is required. Please enter the data required on the questionnaire below.
A free hand sketch of the pipe work with distances to;- bends, pumps, valves etc., should be drawn on the reverse of this data sheet.

	PROCESS AND MEASUREMENT DETAILS

	
	Maximum
	Normal
	Minimum

	Calibration range (SGU)
	
	[bookmark: Text6]     
	
	     
	
	     

	Process temperature (°C)
	
	     
	
	     
	
	     

	Ambient temperature (°C)
	
	     
	
	     
	
	     

	Process material
	
	
	
	     
	
	

	Density of solids (SGU)
	
	
	
	     
	
	

	Density of carrying liquid (SGU)
	
	
	
	     
	
	

	Pipe material
	
	
	
	     
	
	

	Solid Density of Pipe Material
	
	
	[bookmark: Text13]     
	
	

	Pipe outside diameter (mm)
	
	
	
	     
	
	

	Pipe Wall thickness per side (mm)
	
	
	
	     
	
	

	Pipe liner material
	
	
	
	     
	
	

	Solid Density of Pipe Liner Material
	
	
	[bookmark: Text14]     
	
	

	Pipe liner thickness per side (mm)
	
	
	
	     
	
	

	Pipe insulation material
	
	
	
	     
	
	

	Solid Density of Pipe Insulation Material
	
	
	[bookmark: Text15]     
	
	

	Pipe insulation thickness per side (mm)
	
	
	
	     
	
	

	Hazardous location?
	
	|_| Yes   |_| No
	
	     
	
	(Classification)

	Temperature compensation required?
	
	|_| Yes   |_| No
	
	     
	
	(Temp. co-efficient)

	More than one different type of material pumped?
	
	|_| Yes   |_| No
	
	(Mark Choice)
	
	

	Severe vibration?
	
	|_| Yes   |_| No
	
	(Mark Choice)
	
	

	Enclosure protection class
	
	[bookmark: Check3][bookmark: Check4][bookmark: Check5]|_| IP54 (std) |_| IP55 |_| IP 
	
	     
	
	(Mark Choice)

	[image: ][image: ]At the point of density measurement, is the pipeline Vertical or Horizontal? (Vertical Recommended)

	If Vertical Pipeline, is the product flow                                                      |_| Vertical                                 |_| Horizontal
upwards at the point of density measurement ?                                        (Mark Choice)                            (Mark Choice)                                              
 |_| Yes   |_| No   (Mark Choice)

	 

	

	ELECTRONICS REQUIRED

	

	UniproI to Scintillator detector (Blind Unit)
	|_| Yes   |_| No
	(Mark Choice)

	

	Ramsey to Scintillator detector (Blind Unit)
	|_| Yes   |_| No
	(Mark Choice)

	Ronan to Scintillator detector (Blind Unit)
	|_| Yes   |_| No
	(Mark Choice)

	Ohmart to Scintillator detector (Blind Unit)
	|_| Yes   |_| No
	(Mark Choice)

	Krohne to Scintillator detector (Blind Unit)
	|_| Yes   |_| No
	(Mark Choice)

	RTU – Remote Terminal Unit
	|_| Yes   |_| No
	(Mark Choice)

	PTU – Portable Terminal Unit
	|_| Yes   |_| No
	(Mark Choice)

	PTCU – Portable Terminal Connection Unit
	|_| Yes   |_| No
	(Mark Choice)

	Power supply available
	[bookmark: Check6][bookmark: Check7][bookmark: Check10][bookmark: Check8][bookmark: Check9]|_| 220Vac  |_| 110Vac  |_| 24Vac  |_| 50 Hz  |_| 60 Hz
	(Mark Choice)

	OPTIONS

	Special painting?
	[bookmark: Check18][bookmark: Check19]|_| PA Proprietary (Blue)    |_| Galvanized    |_| Other (as per attached)    |_| None   

	Stainless steel sensor set?
	|_| Yes   |_| No
	(Mark Choice)

	Constant voltage transformer required?
	|_| Yes   |_| No
	(Mark Choice)

	Inter-connecting cable (part 2839/100) required?
	|_| Yes   |_| No
	[bookmark: Text9]      Metres
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	SOURCE ON SITE – (DETAILS FROM TAGGING PLATE)

	[bookmark: OLE_LINK1]

	Make: (Source supplied by)
	     
	

	

	Date:
	     
	

	

	Source size:
	     
	

	

	Serial Number:
	     
	

	

	Source type: (CS137/Cobalt)
	     
	

	

	Pipe Clamps: (Sketch if possible)
	     
	

	
	
	

	

	SPECIAL REQUIREMENTS

	

	
	     
	

	
	     
	

	

	

	SKETCH OF PIPING (Side View)

	or alternatively attach a drawing (ACAD .dwg or .pdf format) of the piping

























	

	

	DETAILS - RADIATION PROTECTION OFFICER

	

	Name:
	     
	
	Tel no:
	     
	

	Designation:
	     
	
	Fax no:
	     
	

	E-mail:
	     
	
	

	

	

	CONFIRMATION OF TECHNICAL DETAILS AS SET OUT ABOVE (requirement of ISO 9000/9001)

	

	Print Name:
	     
	
	Designation:
	     
	

	Signature:
	
	
	Date:
	     
	

	

	

	FOR OFFICE USE

	

	Model purchased:
	     
	

	

	Detector type to be supplied:
	     
	

	

	Isotope activity to be supplied:
	     
	

	

	Additional requirements:
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